**Meeting Objectives**

*For TAG members to have the opportunity to achieve consensus on the following:*

* Tiered BUA thresholds for post-construction stormwater requirements, including basic treatment requirements at each
* Volume reduction requirement
* Stream protection criteria
* {possible} Post-construction stormwater treatment requirement applicability trigger

|  |  |
| --- | --- |
| Agenda  |  |
| 10 am  | **Welcome, meeting purpose, introductions, working together**  |
| 10:10 pm *20 minutes*  | **Present, discuss & consensus check on tiered thresholds**  (10 minutes)* Discuss 6%/12% BUA cutoff
* Addition of SCM requirements above 6% or when stormwater collection system is present or proposed

 (10 minutes)* Call to question
* Go-around: your rationale for your vote
 |
| 10:30 am *20 minutes*  | **Present, discuss & consensus check on volume reduction requirement**  (10 minutes)* Applies above 12% BUA or with stormwater collection system
* Optional 90th percentile design storm size without volume reduction
* Incentivizes stormwater recharge

 (10 minutes)* Call to question
* Go-around: your rationale for your vote
 |
| 10:50 am*20 minutes* | **Present, discuss & consensus check on stream protection criteria** (10 minutes)* Applies above 12% BUA
* Protects against prolonged erosive flows
* Exemptions where little to no benefit can be demonstrated
1. inutes)
* Call to question & Go-around: your rationale for your vote
 |
| 11:10 am*30 minutes*  | **Present and discuss applicability trigger*** 1 acre disturbance threshold
* Exemptions
* {Possible} call to question
* Exemptions
 |
| 11:40 am *20 minutes* | **Next steps**  |
| Noon  | **Adjourn** |